

Technical Safety Concept Lane Assistance

**Document Version: [Version]**

**Template Version 1.0, Released on 2017-06-21**



# Document history

**[Instructions: Fill in the date, version and description fields. You can fill out the Editor field with your name if you want to do so. Keep track of your editing as if this were a real world project.**

**For example, if this were your first draft or first submission, you might say version 1.0. If this is a second submission attempt, then you'd add a second line with a new date and version 2.0]**

|  |  |  |  |
| --- | --- | --- | --- |
| Date | Version | Editor | Description |
| 06/23/19 | 1.0 | Adam Gotlib | First draft |
| 06/23/19 | 1.1 | Adam Gotlib |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |

# 

# Table of Contents

**[Instructions: We have provided a table of contents. If the table of contents is not showing up correctly in your word processor of choice, please update it. The table of contents should show each section of the document and page numbers or links. Most word processors can do this for you. In** [**Google Docs**](https://support.google.com/docs/answer/116338?co=GENIE.Platform%3DDesktop&hl=en)**, you can use headings for each section and then go to Insert > Table of Contents.** [**Microsoft Word**](https://support.microsoft.com/en-us/help/285059/how-to-create-a-table-of-contents-by-marking-text-in-word) **has similar capabilities]**

[Document history](#_1t3h5sf)

[Table of Contents](#_ktt3lgighckp)

[Purpose of the Technical Safety Concept](#_fulgh8sf1ocg)

[Inputs to the Technical Safety Concept](#_757cx6xm46zb)

[Functional Safety Requirements](#_2f9rjqxbsp2)

[Refined System Architecture from Functional Safety Concept](#_qp3s9pvua9mt)

[Functional overview of architecture elements](#_cqb49updinx4)

[Technical Safety Concept](#_mx8us8onanqo)

[Technical Safety Requirements](#_lnxjuovv6kca)

[Refinement of the System Architecture](#_74udkdvf7nod)

[Allocation of Technical Safety Requirements to Architecture Elements](#_g2lqf7kmbspk)

[Warning and Degradation Concept](#_4w6r8buy4lrp)

# Purpose of the Technical Safety Concept

**[Instructions: Answer what is the purpose of a technical safety concept?]**

The Technical Safety Concept serves the purpose of deriving more detailed Technical Safety Requirements from the Functional Safety Requirements defined in the Functional Safety Concept.

# Inputs to the Technical Safety Concept

## Functional Safety Requirements

**[Instructions: Provide the functional safety requirements derived in the functional safety concept ]**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **ID** | **Functional Safety Requirement** | **ASIL** | **Fault Tolerant Time Interval** | **Safe State** |
| Functional  Safety  Requirement  01-01 | The lane keeping item shall ensure that the lane departure oscillating torque amplitude is below Max\_Torque\_Amplitude. | C | 50 ms | The LDW function shall deactivate and display a visual warning to the driver. |
| Functional  Safety  Requirement  01-02 | The lane keeping item shall ensure that the lane departure oscillating torque frequency is below Max\_Torque\_Frequency. | C | 50 ms | The LDW function shall deactivate and display a visual warning to the driver. |
| Functional  Safety  Requirement  02-01 | The lane keeping item shall ensure that the lane keeping assistance torque is applied only for Max\_Duratoin. | B | 500 ms | The LKA function shall deactivate and display a visual warning to the driver. |

## Refined System Architecture from Functional Safety Concept

**[Instructions: Provide the refined system architecture from the functional safety concept]**

### 

### Functional overview of architecture elements

**[Instructions: Provide a description for each functional safety element; what is each element's purpose in the lane assistance item? ]**

|  |  |
| --- | --- |
| **Element** | **Description** |
| Camera Sensor | Captures images in front of the vehicle. |
| Camera Sensor ECU - Lane Sensing | Analyses captured images and determines when the vehicle leaves the lane by mistake. |
| Camera Sensor ECU - Torque request generator | Generates lane keeping torque and lane departure oscillating torque request when the vehicle leaves the lane by mistake. |
| Car Display | Displays visual cues for the driver, informing them of functioning of the system. |
| Car Display ECU - Lane Assistance On/Off Status | Displays on/off status of the Lane Assistance item. |
| Car Display ECU - Lane Assistant Active/Inactive | Displays active/inactive status of LDW and LKA functions. |
| Car Display ECU - Lane Assistance malfunction warning | Informs the driver when LDW or LKA malfunction. |
| Driver Steering Torque Sensor | Measures the torque provided by the driver. |
| Electronic Power Steering (EPS) ECU - Driver Steering Torque | Reads the measured torque from the Driver Steering Torque Sensor. |
| EPS ECU - Normal Lane Assistance Functionality | Estimates the required amount of additional torque to be applied based on a lane assistance system torque request and the torque provided by the driver. |
| EPS ECU - Lane Departure Warning Safety Functionality | Ensures that the lane departure oscillating torque amplitude is below Max\_Torque\_Amplitude and the lane departure oscillating torque frequency is below Max\_Torque\_Frequency. |
| EPS ECU - Lane Keeping Assistant Safety Functionality | Ensures that the lane keeping assistance torque is applied only for Max\_Duratoin. |
| EPS ECU - Final Torque | Passes torque request to the Motor. |
| Motor | Applies additional torque to the steering wheel. |

# Technical Safety Concept

## Technical Safety Requirements

**[Instructions: Fill in the technical safety requirements for the lane departure warning first functional safety requirement. We have provided the associated functional safety requirement in the first table below. Hint: The technical safety requirements were discussed in the lesson videos. The architecture allocation column should contain element names such as LDW Safety block, Data Transmission Integrity Check, etc. Allocating the technical safety requirements to the "EPS ECU" does not provide enough detail for a technical safety concept.]**

**Lane Departure Warning (LDW) Requirements:**

Functional Safety Requirement 01-01 with its associated system elements

(derived in the functional safety concept)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **ID** | **Functional Safety Requirement** | **Electronic Power Steering ECU** | **Camera ECU** | **Car Display ECU** |
| Functional  Safety  Requirement  01-01 | The lane keeping item shall ensure that the lane departure oscillating torque amplitude is below Max\_Torque\_Amplitude | X |  |  |

Technical Safety Requirements related to Functional Safety Requirement 01-01 are:

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **ID** | **Technical Safety Requirement** | **ASIL** | **Fault Tolerant Time Interval** | **Architecture Allocation** | **Safe State** |
| Technical  Safety  Requirement  01 | The LDW safety compontent shall ensure that the amplitude of the LDW\_Torque\_Request sent to the Final EPS Torque component is below Max\_Torque\_Amplitude. | C | 50 ms | LDW Safety Functionality | The LDW function shall deactivate and display a visual warning to the driver. |
| Technical  Safety  Requirement  02 | The validity and integrity of the data transmission for LDW\_Torque\_Request signal shall be ensured. | C | 50 ms | LDW Safety Functionality | The LDW function shall deactivate and display a visual warning to the driver. |
| Technical  Safety  Requirement  03 | As soon as a failure is detected by the LDW function, it shall deactiveate the LDW feature and the LDW\_Torque\_Request shall be set to zero. | C | 50 ms | LDW Safety Functionality | The LDW function shall deactivate and display a visual warning to the driver. |
| Technical  Safety  Requirement  04 | As soon as the LDW function deactivates the LDW feature the LDW Safety software block shall send a signal to the Car Display ECU to turn on a warning light. | C | 50 ms | LDW Safety Functionality | The LDW function shall deactivate and display a visual warning to the driver. |
| Technical  Safety  Requirement  05 | Memory test shall be conducted at start up of the EPS ECU to check for any faults in memory. | A | Ignition cycle | LDW Safety Functionality | The LDW function shall deactivate and display a visual warning to the driver. |

**[Instructions: Fill in the technical safety requirements for the lane departure warning second functional safety requirement. We have provided the associated functional safety requirement in the table below. Hint:. Most of the technical safety requirements will be the same. At least one technical safety requirement will have to be slightly modified because we are talking about frequency instead of amplitude. These requirements were not given in the lessons]**

Functional Safety Requirement 01-2 with its associated system elements

(derived in the functional safety concept)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **ID** | **Functional Safety Requirement** | **Electronic Power Steering ECU** | **Camera ECU** | **Car Display ECU** |
| Functional  Safety  Requirement  01-02 | The lane keeping item shall ensure that the lane departure oscillating torque frequency is below Max\_Torque\_Frequency | X |  |  |

Technical Safety Requirements related to Functional Safety Requirement 01-02 are:

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **ID** | **Technical Safety Requirement** | **ASIL** | **Fault Tolerant Time Interval** | **Architecture Allocation** | **Safe State** |
| Technical  Safety  Requirement  01 | The LDW safety compontent shall ensure that the frequency of the LDW\_Torque\_Request sent to the Final EPS Torque component is below Max\_Torque\_Frequency | C | 50 ms | LDW Safety Functionality | The LDW function shall deactivate and display a visual warning to the driver. |
| Technical  Safety  Requirement  02 | The validity and integrity of the data transmission for LDW\_Torque\_Request signal shall be ensured. | C | 50 ms | LDW Safety Functionality | The LDW function shall deactivate and display a visual warning to the driver. |
| Technical  Safety  Requirement  03 | As soon as a failure is detected by the LDW function, it shall deactiveate the LDW feature and the LDW\_Torque\_Request shall be set to zero. | C | 50 ms | LDW Safety Functionality | The LDW function shall deactivate and display a visual warning to the driver. |
| Technical  Safety  Requirement  04 | As soon as the LDW function deactivates the LDW feature the LDW Safety software block shall send a signal to the Car Display ECU to turn on a warning light. | C | 50 ms | LDW Safety Functionality | The LDW function shall deactivate and display a visual warning to the driver. |
| Technical  Safety  Requirement  05 | Memory test shall be conducted at start up of the EPS ECU to check for any faults in memory. | A | Ignition cycle | LDW Safety Functionality | The LDW function shall deactivate and display a visual warning to the driver. |

**Lane Departure Warning (LDW) Verification and Validation Acceptance Criteria:**

**[OPTIONAL: For each technical safety requirement, identify both the verification and validation acceptance criteria. “Validation” asks whether or not you chose the appropriate parameters. “Verification” involves testing to make sure the vehicle behaves as expected when the parameter value is crossed. There is not necessarily one right answer. Look at your verification and validation acceptance criteria from the functional safety concept for inspiration.]**

**Lane Keeping Assistance (LKA) Requirements:**

**[Instructions: Fill in the technical safety requirements for the lane keeping assistance functional safety requirement 02-01. We have provided the associated functional safety requirement in the table below. Hint:. You can reuse the technical safety requirements from functional safety requirement 01-01. But you need to change the language because we are now looking at a different system. The ASIL and Fault Tolerant Time Interval are different as well.]**

Functional Safety Requirement 02-1 with its associated system elements

(derived in the functional safety concept)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **ID** | **Functional Safety Requirement** | **Electronic Power Steering ECU** | **Camera ECU** | **Car Display ECU** |
| Functional  Safety  Requirement  02-01 | The lane keeping item shall ensure that the lane keeping assistance torque is applied for only Max\_Duration | X |  |  |

Technical Safety Requirements related to Functional Safety Requirement 02-01 are:

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **ID** | **Technical Safety Requirement** | **ASIL** | **Fault Tolerant Time Interval** | **Allocation to Architecture** | **Safe State** |
| Technical  Safety  Requirement  01 | The LKA safety compontent shall ensure that the LKA\_Torque\_Request sent to the Final EPS Torque component has non-zero value for only Max\_Duration. | B | 500 ms | LKA Safety Functionality | The LKA function shall deactivate and display a visual warning to the driver. |
| Technical  Safety  Requirement  02 | The validity and integrity of the data transmission for LKA\_Torque\_Request signal shall be ensured. | B | 500 ms | LKA Safety Functionality | The LKA function shall deactivate and display a visual warning to the driver. |
| Technical  Safety  Requirement  03 | As soon as a failure is detected by the LKA function, it shall deactiveate the LKA feature and the LKA\_Torque\_Request shall be set to zero. | B | 500 ms | LKA Safety Functionality | The LKA function shall deactivate and display a visual warning to the driver. |
| Technical  Safety  Requirement  04 | As soon as the LKA function deactivates the LKA feature the LKA Safety software block shall send a signal to the Car Display ECU to turn on a warning light. | B | 500 ms | LKA Safety Functionality | The LKA function shall deactivate and display a visual warning to the driver. |
| Technical  Safety  Requirement  05 | Memory test shall be conducted at start up of the EPS ECU to check for any faults in memory. | A | Ignition cycle | LKA Safety Functionality | The LKA function shall deactivate and display a visual warning to the driver. |

**Lane Keeping Assistance (LKA) Verification and Validation Acceptance Criteria:**

**[OPTIONAL: For each technical safety requirement, identify both the verification and validation acceptance criteria. “Validation” asks whether or not you chose the appropriate parameters. “Verification” involves testing to make sure the vehicle behaves as expected when the parameter value is crossed. There is not necessarily one right answer. Look at your verification and validation acceptance criteria from the functional safety concept for inspiration.]**

## Refinement of the System Architecture

**[Instructions: Include the refined system architecture. Hint: The refined system architecture should include the system architecture from the end of the technical safety lesson, including all of the ASIL labels.]**

****

## Allocation of Technical Safety Requirements to Architecture Elements

**[Instructions: We already included the allocation as part of the technical requirement tables. Here you can state that for this particular item, all technical safety requirements are allocated to the Electronic Power Steering ECU]**

For this particular item, all technical safety requirements are allocated to the EPS ECU component.

## Warning and Degradation Concept

**[Instructions: We've already identified that for any system malfunction, the lane assistance functions will be turned off and the driver will receive a warning light indication. The technical safety requirements have not changed how functionality will be degraded or what the warning will be.**

**So in this case, the warning and degradation concept is the same for the technical safety requirements as for the functional safety requirements. You can copy the functional safety warning and degradation concept here.**

**Oftentimes, a technical safety analysis will lead to a more detailed warning and degradation concept. ]**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **ID** | **Degradation Mode** | **Trigger for Degradation Mode** | **Safe State invoked?** | **Driver Warning** |
| WDC-01 | Deactivate LDW function. | Malfunction\_01  Malfunction\_02 | YES | Visual display |
| WDC-02 | Deactivate LKA function. | Malfunction\_03 | YES | Visual display |